Tile e084n21
Location (Lat,Long): 21°N, 84°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 45
Tile center (UTM: X,Y): 188106.92493, 2325075.69452 m
Upper left corner (UTM: X,Y): 178086.92493, 2335095.69452 m
Lower right corner (UTM: X,Y): 198126.92493, 2315055.69452 m

Landsat platform/sensor: 5/TM
WRS2 Path: 141; Row: 045
Date: 1989/10/31
Landsat data within tile: 100.000 %
Landsat cloud cover within tile: 0.003 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 15 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e084n21.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
