Tile e111n51
Location (Lat,Long): 51°N, 111°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 49
Tile center (UTM: X,Y): 500000.00000, 5649824.88870 m
Upper left corner (UTM: X,Y): 489980.00000, 5659844.88870 m
Lower right corner (UTM: X,Y): 510020.00000, 5639804.88870 m

Landsat platform/sensor: 4/TM
WRS2 Path: 129; Row: 025
Date: 1990/05/15
Landsat data within tile: 85.409 %
Landsat cloud cover within tile: 4.007 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 60 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e111n51.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
