Tile e125n06
Location (Lat,Long): 6°N, 125°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 51
Tile center (UTM: X,Y): 721383.14550, 663608.57533 m
Upper left corner (UTM: X,Y): 711363.14550, 673628.57533 m
Lower right corner (UTM: X,Y): 731403.14550, 653588.57533 m

Landsat platform/sensor: 4/TM
WRS2 Path: 112; Row: 056
Date: 1989/12/31
Landsat data within tile: 100.000 %
Landsat cloud cover within tile: 0.769 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 15 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e125n06.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
