Tile e047n55
Location (Lat,Long): 55°N, 47°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 38
Tile center (UTM: X,Y): 627928.19138, 6096620.70708 m
Upper left corner (UTM: X,Y): 617908.19138, 6106640.70708 m
Lower right corner (UTM: X,Y): 637948.19138, 6086600.70708 m

Landsat platform/sensor: 7/ETM+
WRS2 Path: 171; Row: 022
Date: 2000/09/05
Landsat data within tile: 99.370 %
Landsat cloud cover within tile: 0.000 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 30 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e047n55.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
