Tile e078n18
Location (Lat,Long): 18°N, 78°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 44
Tile center (UTM: X,Y): 182293.88637, 1992757.47283 m
Upper left corner (UTM: X,Y): 172273.88637, 2002777.47283 m
Lower right corner (UTM: X,Y): 192313.88637, 1982737.47283 m

Landsat platform/sensor: 7/ETM+
WRS2 Path: 144; Row: 048
Date: 2001/10/29
Landsat data within tile: 100.000 %
Landsat cloud cover within tile: 0.000 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e078n18.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
