Tile e138s08
Location (Lat,Long): 8°S, 138°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 54
Tile center (UTM: X,Y): 169256.15771, -885503.75930 m
Upper left corner (UTM: X,Y): 159236.15771, -875483.75930 m
Lower right corner (UTM: X,Y): 179276.15771, -895523.75930 m

Landsat platform/sensor: 7/ETM+
WRS2 Path: 102; Row: 065
Date: 2001/05/16
Landsat data within tile: 98.829 %
Landsat cloud cover within tile: 24.159 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 30 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e138s08.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
