Tile e011n03
Location (Lat,Long): 3°N, 11°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 32
Tile center (UTM: X,Y): 722292.16924, 331796.29168 m
Upper left corner (UTM: X,Y): 712272.16924, 341816.29168 m
Lower right corner (UTM: X,Y): 732312.16924, 321776.29168 m

Landsat platform/sensor: 7/ETM+
WRS2 Path: 185; Row: 058
Date: 2005/11/08
Landsat data within tile: 59.769 %
Landsat cloud cover within tile: 10.752 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 60 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e011n03.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
