Tile e046n44
Location (Lat,Long): 44°N, 46°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 38
Tile center (UTM: X,Y): 580174.25984, 4872358.88566 m
Upper left corner (UTM: X,Y): 570154.25984, 4882378.88566 m
Lower right corner (UTM: X,Y): 590194.25984, 4862338.88566 m

Landsat platform/sensor: 7/ETM+
WRS2 Path: 169; Row: 030
Date: 2007/06/23
Landsat data within tile: 99.972 %
Landsat cloud cover within tile: 0.000 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e046n44.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
