Tile e064n37
Location (Lat,Long): 37°N, 64°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 41
Tile center (UTM: X,Y): 588977.32443, 4095339.69127 m
Upper left corner (UTM: X,Y): 578957.32443, 4105359.69127 m
Lower right corner (UTM: X,Y): 598997.32443, 4085319.69127 m

Landsat platform/sensor: 7/ETM+
WRS2 Path: 156; Row: 034
Date: 2005/06/22
Landsat data within tile: 99.866 %
Landsat cloud cover within tile: 0.000 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e064n37.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
