Tile w135n58
Location (Lat,Long): 58°N, 135°W
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 8
Tile center (UTM: X,Y): 500000.00000, 6428710.15963 m
Upper left corner (UTM: X,Y): 489980.00000, 6438730.15963 m
Lower right corner (UTM: X,Y): 510020.00000, 6418690.15963 m

Landsat platform/sensor: 5/TM
WRS2 Path: 057; Row: 020
Date: 2006/07/29
Landsat data within tile: 100.000 %
Landsat cloud cover within tile: 0.067 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 60 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/w135n58.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
