Tile w156n62
Location (Lat,Long): 62°N, 156°W
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 5
Tile center (UTM: X,Y): 342908.28983, 6877812.60181 m
Upper left corner (UTM: X,Y): 332888.28983, 6887832.60181 m
Lower right corner (UTM: X,Y): 352928.28983, 6867792.60181 m

Landsat platform/sensor: 5/TM
WRS2 Path: 074; Row: 016
Date: 2006/07/04
Landsat data within tile: 100.000 %
Landsat cloud cover within tile: 0.054 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 30 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/w156n62.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
