Tile e022n46
Location (Lat,Long): 46°N, 22°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 34
Tile center (UTM: X,Y): 577432.18257, 5094533.59139 m
Upper left corner (UTM: X,Y): 567412.18257, 5104553.59139 m
Lower right corner (UTM: X,Y): 587452.18257, 5084513.59139 m

Landsat platform/sensor: 5/TM
WRS2 Path: 185; Row: 028
Date: 1988/08/29
Landsat data within tile: 100.000 %
Landsat cloud cover within tile: 0.012 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 60 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e022n46.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
