Tile w126n58
Location (Lat,Long): 58°N, 126°W
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 10
Tile center (UTM: X,Y): 322707.88006, 6432647.78031 m
Upper left corner (UTM: X,Y): 312687.88006, 6442667.78031 m
Lower right corner (UTM: X,Y): 332727.88006, 6422627.78031 m

Landsat platform/sensor: 5/TM
WRS2 Path: 051; Row: 020
Date: 1988/09/03
Landsat data within tile: 97.846 %
Landsat cloud cover within tile: 0.032 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_norm.tif		Normalized image (based on 30 % tree canopy cover threshold)
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/w126n58.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
