Tile e066n35
Location (Lat,Long): 35°N, 66°E
Data format: GeoTIFF
Pixel size: 30 m
Pixels/Lines: 668 x 668
Tile size: 20040 x 20040 m
Projection: UTM, zone 42
Tile center (UTM: X,Y): 226201.90361, 3877156.69171 m
Upper left corner (UTM: X,Y): 216181.90361, 3887176.69171 m
Lower right corner (UTM: X,Y): 236221.90361, 3867136.69171 m

Landsat platform/sensor: 7/ETM+
WRS2 Path: 155; Row: 036
Date: 2006/06/02
Landsat data within tile: 100.000 %
Landsat cloud cover within tile: 1.313 %

Files:
b1_* ... b7_*	Landsat bands 1 ... 7
*_dn.tif		Original Landsat data
*_enh.tif		Histogram enhanced image
cloud_mask.tif	Cloud mask (200 - detected clouds, 100 - buffer pixels)
data_mask.tif	Data mask (100 - Landsat data exist)
pan.tif			band 8 (spatial resolution 15m, only for ETM+ data)

Please, refer to included Landsat metadata (landsat.met) file for additional information
Additional metadata and imagery:
http://globalmonitoring.sdstate.edu/projects/fao/search/e066n35.html

-----------------------------------------------------------------------------------------------
Data source: FAO FRA Landsat Imagery Database
http://globalmonitoring.sdstate.edu/projects/fao/index.html
